Rear License Plate Lamp Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws which secure the license plate lamp assembly.
2. Remove the license plate lamp assembly (2) from the rear door.
3. Remove the license plate lamp bulb socket from the lamp assembly (2).
4. Remove the license plate lamp bulb (1) from the license plate lamp bulb socket.

### Installation Procedure

1. Install the license plate lamp bulb (1) to the license plate lamp bulb socket.
2. Install the license plate lamp bulb socket to the lamp assembly (2).
3. Install the license plate lamp assembly (2) to the rear door. Secure the license plate lamp assembly (2) with the 2 screws.