Instrument Cluster Bulb Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster assembly. Refer to Instrument Cluster Replacement .
2. Remove the bulb sockets from the back of the cluster assembly (18) as needed.
3. Remove the bulbs from the sockets, as needed.

### Installation Procedure

1. Install the bulbs to the bulb sockets, as needed.
2. Install the bulb sockets to the back of the cluster assembly (18), as needed.
3. Install the instrument panel cluster assembly. Refer to Instrument Cluster Replacement .