Power Windows Description. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

You may operate the right front, left rear and right rear windows by two separate switches. The right front window switch is located in the left front power window/door lock switch and in the right front door. The left and right rear remote power window switches are located in the center console, while the individual rear switches are located on each rear door. The window motor stops once the window opens completely or whenever the window switch is released.

In order to close the left rear or the right rear window, lift the appropriate window switch in the left front power window/door lock switch or the center console.

The left front power window/door lock switch also contains the AUTO DOWN and WINDOW LOCK features. The AUTO DOWN feature allows the left front window to open automatically to the fully open position. The WINDOW LOCK feature allows the right front, left rear and right rear windows to be locked out. When you depress the window lock switch, only the left front window switch in the left front power window/door lock switch is operational.