Audio Alarm Module Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

The audio alarm module mounts inside the instrument panel, between the radio and the instrument panel compartment.

### Removal Procedure

1. Pull out the instrument panel compartment while pushing the panel stoppers from both the left and right sides.
2. Disconnect the electrical connector from the audio alarm module (1).
3. Use a flat-bladed screwdriver in order to release the locking tab and remove the audio alarm module (1) from the bracket.

### Installation Procedure

1. Install the audio alarm module (1) to the instrument panel bracket.
2. Connect the electrical connector to the audio alarm module (1).
3. Close the instrument panel compartment.