Instrument Panel Compartment Door Latch Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Pull out the instrument panel compartment while pushing the stopper from both the left and right sides.
2. Remove the 2 screws and the lock assembly from the instrument panel compartment.

### Installation Procedure

1. Install the lock assembly to the instrument panel compartment. Secure the lock assembly with the 2 screws.
2. Close the instrument panel compartment.