Power and Grounding Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Amplifier | Behind the RH instrument panel on the evaporator | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Compressor Clutch Relay | RH engine compartment near fuse block 1 | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Condenser Fan | Between the grille and the radiator | HVAC Component Views in HVAC System - Manual | --
A/C Condenser Fan Relay | RH engine compartment near fuse block 1 | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Switch | Center of the instrument panel above the radio | Power Door Systems Component Views in Doors | --
Airbag Fuse Box | Under the left hand instrument panel near fuse block 2 | -- | --
Antilock Brake System (ABS) Motor Pack Assembly | LH rear engine compartment | Antilock Brake System Component Views in ABS | --
Antilock Brake System (ABS) Resistor | RH instrument panel, behind the instrument panel compartment taped to the main harness | Antilock Brake System Component Views in ABS | --
Audio Alarm Module | Behind the RH instrument panel near the RH front speaker | Entertainment Component Views in Entertainment | --
Battery | RH rear engine compartment behind the strut | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
Backup Lamp Switch (Manual Transmission) | Mounted on the top of the transmission | -- | --
Blower Motor | Behind the RH instrument panel | HVAC Component Views in HVAC System - Manual | --
Blower Speed Selector Switch | Center of the instrument panel above the radio | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
Brake Fluid Level Switch | LH rear of the engine compartment in the brake F1 | Engine Controls Component Views in Engine Controls | --
Cigar Lighter | Center of the instrument panel below the radio | Power Door Systems Component Views in Doors | --
Clutch Pedal Position (CPP) Interrupt Switch (Manual Transmission with Cruise Control) | Under the LH instrument panel mounted to the clutch pedal bracket | Cruise Control Component Views in Cruise Control | --
Combination Switch | On the steering column | -- | --
Cruise Control Actuator | RH engine compartment near the strut tower | Cruise Control Component Views in Cruise Control | --
Cruise Control ON/OFF Switch | LH instrument panel to the right of the steering column | Cruise Control Component Views in Cruise Control | --
Cruise Control Mode Switch | RH steering column on the combination switch | -- | --
Data Link Connector - On Board Diagnostics II (DLC-OBD) | LH instrument panel to the left of the center console of the knee bolster | Power Door Systems Component Views in Doors | Data Link Communications Connector End Views
Daytime Running Lamps (DRL) Control Module | Behind the instrument panel to the left of the steering column on the powertrain module mounting bracket | Lighting Systems Component Views in Lighting Systems | --
Daytime Running Lamps (DRL) Diode | RH instrument panel taped to the main harness above the blower | Lighting Systems Component Views in Lighting Systems | --
Distributor | Top rear of the engine | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Dual Pressure Switch | RH front engine compartment behind the radiator | HVAC Component Views in HVAC System - Manual | --
Duty Check Data Link Connector (DLC) 1 | RH engine compartment behind the RH headlamp | Data Link Communications Component Views | --
Electronic Brake Control Module (EBCM) (with ABS) | Under the LH instrument panel to the right of the steering column | Antilock Brake System Component Views in ABS | --
C1 (32 Cavities) | Main harness to the EBCM behind the instrument panel to the right of the steering column | -- | --
C2 (2 Cavities) | Main harness to the EBCM behind the instrument panel to the right of the steering column | -- | --
Electronic Brake Control Relay | LH engine compartment mounted to the left inner fender in front of the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
Four Wheel Drive Low Switch (4-speed automatic transmission) | Top of the transfer case | -- | --
Four Wheel Drive Switch (4-speed automatic transmission) | Top of the transfer case | -- | --
Four Wheel Drive Switch (manual transmission) | Top of the transfer case | Antilock Brake System Component Views in ABS | --
Front Washer Pump | RH front of the engine compartment on washer F1 | Wiper/Washer Component Views in Wipers/ Washer System | --
Front Wiper Motor | LH rear engine compartment on the bulkhead | Wiper/Washer Component Views in Wipers/ Washer System | --
Fuel Level Sensor | In the fuel tank | Engine Controls Component Views in Engine Controls - 1.6L | --
Fuel Pump | In the fuel tank | Engine Controls Component Views in Engine Controls - 1.6L | --
Fuel Pump Relay | Center of the instrument panel behind the blower speed selector | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Fuse Block 1 | RH engine compartment in front of the battery | Power and Grounding Component Views in wiring systems | --
C1 (3 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in wiring systems | --
C2 (1 Cavities) | A/C harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in wiring systems | --
C3 (1 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in wiring systems | --
C4 (2 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in wiring systems | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in wiring systems | --
Generator | RH lower front of the engine | -- | --
Headlamp Relay 1 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views in Lighting Systems | --
Headlamp Relay 2 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views in Lighting Systems | --
Heated Oxygen Sensor 1 (HO2S1) | LH rear of the engine in the exhaust manifold | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Heated Oxygen Sensor 2 (HO2S2) | Below the vehicle after the 3-way catalytic converter (TWC) | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Horn Relay | Center instrument panel behind the blower speed selector | Horn Component Views in Horns | --
Ignition Key Warning Switch | RH side of the steering column on the ignition switch | -- | --
Ignition Switch | On the steering column | Power and Grounding Component Views in wiring systems | --
Illumination Controller | LH instrument panel to the left of the steering column | -- | --
Inflatable Restraint I/P Module | Top of the RH instrument panel above the instrument panel compartment | Power Door Systems Component Views in Doors | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Under the center of the instrument panel | Power Door Systems Component Views in Doors | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C1 (16 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C2 (10 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
Lamp Driver Relay | LH engine compartment mounted to the left inner fender in the front of the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
Left Horn | Between the grille and the radiator | Wiper/Washer Component Views in Wipers/ Washer Systems | --
LH Door Jamb Switch (2 Door) | Lower the LH B-Pillar | Lighting Systems Component Views in Lighting Systems | --
LH Front ABS Solenoid | LH rear engine compartment attached to the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
LH Front Door Jamb Switch (4-Door) | Lower LH B-Pillar | Lighting Systems Component Views in Lighting Systems | --
LH Front Power Door Lock Actuator Assembly (4-Door) | LH front power door on the door latch assembly | Power Door Systems Component Views in Doors | --
C1 (3 Cavities) | LH front door, LH front door harness to the LH front power door latch actuator | -- | --
C2 (6 Cavities | LH front door, LH front door harness to the LH front power door latch actuator | -- | --
LH Front Power Window/ Door Lock Switch (4-Door) | LH front door in the armrest | -- | --
LH Rear Door Jamb Switch (4-Door) | LH C-Pillar above the wheelhousing | Lighting Systems Component Views in Lighting Systems | --
LH Rear Remote Power Window Switch (4-Door) | LH rear of center console | Power Door Systems Component Views in Doors | --
Main Relay | Center of the instrument panel behind the blower speed selector | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Mass Air Flow (MAF) Sensor | LH front engine compartment on the air cleaner (ACL) housing | Engine Controls Component Views in Engine Controls - 1.6L | Engine Controls Component Views in Engine Controls - 1.6L
Noise Suppressor Filter | LH rear engine compartment below the front wiper motor | Engine Controls Component Views in Engine Controls - 1.6L | Engine Controls Component Views in Engine Controls - 1.6L
Overdrive Switch (4-Speed Automatic Transmission) | Center console mounted in the manual selector lever | -- | --
Park/ Neutral Position (PNP) Switch (3-Speed Automatic Transmission) | RH side of the transmission | -- | --
C1 (2 Cavities) | Engine harness to PNP switch on RH side of the transmission | -- | --
C2 (4 Cavities) | Engine harness to PNP switch on the RH side of the transmission | -- | --
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls - 1.6L | Engine Controls Component Views in Engine Controls - 1.6L
3-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C3 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
4-Speed Automatic and Manual Transmissions C4 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
Power Door Lock Control Module (4-Door) | LH instrument panel behind the power mirror switch to the left of the steering column | Power Door Systems Component Views in Doors | --
Power Mirror Switch (4-Door) | LH instrument panel to the left of the steering column | Power Door Systems Component Views in Doors | --
Power/ Normal Switch (4-Speed Automatic Transmission) | In the center console to the right of the manual selector lever | -- | --
Power Windows Circuit Breaker (4-Door) | LH instrument panel mounted to fuse block 2 | -- | --
Radio | Center of the instrument panel | Power Door Systems Component Views in Doors | --
Rear Defogger (4-Door) | In the rear window | -- | --
Rear Defogger Switch (4-Door) | LH instrument panel to the left of the steering column | -- | --
Rear Door Jamb Switch | LH bottom of the rear door jamb | Power Door Systems Component Views in Doors | --
Rear Door Power Door Lock Actuator Assembly (4-Door) | Rear door on the door latch assembly | -- | --
Rear Washer Pump (4-Door) | RH front engine compartment on the washer fluid reservoir | Wiper/Washer Component Views in Wipers/ Washers System | --
Rear Wiper Motor (4-Door) | In the center of the rear door | Wiper/Washer Component Views in Wipers/ Washers System | --
Rear Wiper/ Washer Switch (4-Door) | LH instrument panel to the right of the steering column | Power and Grounding Component Views in wiring systems | --
RH Door Jamb Switch (2-Door) | Lower RH B-pillar | Power Door Systems Component Views in Doors | --
RH Front ABS Solenoid | LH rear engine compartment attached to the ABS Hydraulic Motor Pack Assembly | Antilock Brake System Component Views in ABS | --
RH Front Door Jamb Switch (4-Door) | Lower RH B-pillar | -- | --
RH Front Power Door Lock Actuator Assembly (4-Door) | RH front door on the door latch assembly | -- | --
C1 (3 Cavities) | RH front door harness to the RH front power door lock actuator | Power Door Systems Component Views in Doors | --
RH Front Power Window Switch (4-Door) | RH front door in the armrest | -- | --
RH Rear Door Jamb (4-Door) | RH C-pillar above the wheelhousing | -- | --
RH Rear Power Window Switch (4-Door) | RH rear door behind the trim panel near the armrest | Power Door Systems Component Views in Doors | --
RH Rear Remote Power Window (4-Door) | RH rear of the center console | Power Door Systems Component Views in Doors | --
Seat Belt Switch | In the driver seat belt buckle on the driver's seat adjuster | -- | --
Shift Lock Relay (Automatic Transmission) | RH engine compartment in front of the battery | -- | --
Shift Lock Solenoid (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Shift Lock Solenoid Capacitor (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Shuttle Switch | LH rear engine compartment attached to the ABS hydraulic motor pack assembly | -- | --
Starter Motor | Lower RH side of the engine under the intake manifold | -- | --
Starter Solenoid | Lower RH side of the engine on the starter motor | -- | --
Stoplamp Switch | Under the LH instrument panel above the brake pedal | Lighting Systems Component Views in Lighting Systems | --
Supplemental Inflatable Restraint (SIR) Data Link Connector (DLC) | LH instrument panel under the steering column | Power Door Systems Component Views in Doors | --
Torque Converter Clutch (TCC) Relay (3-Speed Automatic Transmission) | RH engine compartment in front of the battery | -- | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of the transmission | -- | --
Turn/ Hazard Relay | Center instrument panel behind the blower speed selector | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
C100 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C101 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C102 (6 Cavities) (3-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C102 (4 Cavities) (Manual and 4-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C103 (12 Cavities) (Manual and 4-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in wiring systems | --
C104 (6 Cavities) (Manual and 3-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in wiring systems | --
C104 (9 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in wiring systems | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in wiring systems | --
C108 (4 Cavities) | Main harness to the A/C sub-harness behind the RH headlamp | Harness Routing Views in wiring systems | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in wiring systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in wiring systems | --
C202 (22 Cavities) | Main harness to the floor harness, LH instrument panel near G200 | Harness Routing Views in wiring systems | --
C205 (4 Cavities) (4-Door) | Main harness to the LH front door harness, LH instrument panel near the A-pillar | Harness Routing Views in wiring systems | --
C207 (4 Cavities) (4-Door) | Main harness to the RH front door harness, RH instrument panel near the A-pillar | Harness Routing Views in wiring systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in wiring systems | --
C212 (10 Cavities) | Main harness to the A/C amplifier jumper harness, RH instrument panel behind the instrument panel compartment | Harness Routing Views in wiring systems | --
C213 (6 Cavities) | Instrument panel harness to the shift illumination | Harness Routing Views in wiring systems | --
C215 (2 Cavities) (4-Door) | Main harness to the dome lamp harness, RH instrument panel near the A-pillar | Harness Routing Views in wiring systems | --
C300 (2 Cavities) (2-Door) | Floor harness to the dome lamp harness behind the LH rear passenger compartment trim panel | Harness Routing Views in wiring systems | --
C301 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views in wiring systems | --
C305 (3 Cavities) (4-Door) | Floor harness to the LH rear door harness, LH B-pillar | Harness Routing Views in wiring systems | --
C306 (3 Cavities) (4-Door) | Floor harness to the RH rear door harness, RH B-pillar | Harness Routing Views in wiring systems | --
C400 (12 Cavities) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views in wiring systems | --
C402 (6 Cavities) | Rear lamp harness to the RH rear combination lamp jumper harness behind the RH rear wheelhousing | Harness Routing Views in wiring systems | --
C404 (1 Cavity) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in wiring systems | --
C405 (2 Cavities) (4-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the rear door to the left of the license plate lamp connector breakout | Harness Routing Views in wiring systems | --
C405 (2 Cavities) (2-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the center rear door | Harness Routing Views in wiring systems | --
C406 (6 Cavities) | Floor harness to the LH rear combination lamp jumper harness behind the LH rear wheelhousing | Harness Routing Views in wiring systems | --
C407 (6 Cavities) | Floor harness to the trailer option harness behind the LH rear wheelhousing | Harness Routing Views in wiring systems | --
C408 (3 Cavities) (4-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views in wiring systems | --
C500 (10 Cavities) (4-Door) | LH front door harness to the LH front door power accessory harness in the LH front door right of the handle | Harness Routing Views in wiring systems | --
C600 (10 Cavities) (4-Door) | RH front door harness to the RH front door power accessory harness in the RH front door to the left of the handle | Harness Routing Views in wiring systems | --
C601 (4 Cavities) (4-Door) | RH front door power accessory harness to the RH front power window jumper harness in the RH front door left of the handle | Harness Routing Views in wiring systems | --
C700 (4 Cavities) (4-Door) | LH rear door, center of door behind armrest | Harness Routing Views in wirng systems | --
C800 (4 Cavities) (4-Door) | RH rear door, center of door behind armrest | Harness Routing Views in wiring systems | --
G100 | LH front inner fender | Power and Grounding Component Views in wiring systems | --
G101 | On the bulkhead behind the distributor | Power and Grounding Component Views in wiring systems | --
G102 | RH rear of the engine near the distributor | Power and Grounding Component Views in wiring systems | --
G103 | RH rear engine compartment mounted to the intake manifold | Power and Grounding Component Views in wiring systems | --
G104 | RH front inner fender near the washer fluid reservoir | Power and Grounding Component Views in wiring systems | --
G105 (with ABS) | RH inner fender near the battery | Power and Grounding Component Views in wiring systems | --
G106 | RH inner fender near the battery | Power and Grounding Component Views in wirng systems | --
G107 | RH engine near the starter motor | Power and Grounding Component Views in wiring systems | --
G108 (with A/C) | RH inner fender near the battery | Power and Grounding Component Views in wiring systems | --
G109 | LH bulkhead near the front of the wiper motor | Power and Grounding Component Views in wiring systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in wiring systems | --
G201 | Behind the RH instrument panel near the blower assembly | Power and Grounding Component Views in wiring systems | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views in wiring systems | --
G203 | Center instrument panel on the sensing and diagnostic module mounting bracket | Power and Grounding Component Views in wiring systems | --
G300 (4-Door) | LH rear passenger compartment behind the trim panel | Power and Grounding Component Views in wiring systems | --
G300 (2-Door) | LH rear passenger compartment behind the trim plate | Power and Grounding Component Views in wiring systems | --
G400 (4-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in wiring systems | --
G400 (2-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views in wiring systems | --
G401 (4-Door) | Rear door harness near the rear wiper motor on the door | Power and Grounding Component Views in wiring systems | --
G402 (2-Door) | Rear lamp harness behind the LH rear wheelhousing | Power and Grounding Component Views in wiring systems | --
G403 (4-Door) | Rear door harness near the rear wiper motor on the mounting bracket | Power and Grounding Component Views in wiring systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Harness Routing Views in wiring systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Harness Routing Views in wiring systems | --
P300 (2-Door) | LH A-pillar under the instrument panel behind the LH kick panel | Harness Routing Views in wiring systems | --
P400 (2-Door) | Rear door | Harness Routing Views in wiring systems | --
P400 (4-Door) | Rear door | Harness Routing Views in wiring systems | --
P401 | Rear of the vehicle to the right of the LH frame rail | Harness Routing Views in wiring systems | --
P402 | Rear of the vehicle to the left of the RH frame rail | Harness Routing Views in wiring systems | --
P500 (4-Door) | LH front door | Harness Routing Views in wiring systems | --
P600 (4-Door) | RH front door | Harness Routing Views in wiring systems | --
P700 (4-Door) | LH rear door | Harness Routing Views in wiring systems | --
P800 (4-Door) | RH rear door | Harness Routing Views in wiring systems | --
S103 | Main harness approximately 8 cm (3.14 in) from the right horn connectors breakout | Harness Routing Views in wiring systems | --
S104 | Main harness approximately 4 cm (1.57 in) from the front washer pump connector breakout | Harness Routing Views in wiring systems | --
S106 | Main harness, approximately 10 cm (3.93 in) from the noise suppressor filter connector breakout | Harness Routing Views in wiring systems | --
S107 | Engine harness approximately 10 cm (3.93 in) from the C104 breakout | Harness Routing Views in wiring systems | --
S108 (4-Speed Automatic Transmission) | Transmission harness near 4WD switch breakout | Harness Routing Views in wiring systems | --
S110 | Outer A/C harness RH engine compartment near the strut tower | Harness Routing Views in wiring systems | --
S115 | Main harness approximately 10 cm (3.93 in) from the evaporative canister vent control valve | Harness Routing Views in wiring systems | --
S116 | Main harness approximately 14 cm (5.51 in) from the LH bulkhead branch breakout | Harness Routing Views in wiring systems | --
S120 | Main harness approximately 15 cm (5.90 in) from the G100 breakout | Harness Routing Views in wiring systems | --
S130 | Main harness approximately 20 cm (7.87 in) from the noise suppressor filter connector breakout | Harness Routing Views in wiring systems | --
S131 | Main harness approximately 19 cm (7.48 in) from P201 | Harness Routing Views in wiring systems | --
S132 | Main harness approximately 7 cm (2.75 in) from the noise suppressor filter connector breakout | Harness Routing Views in wiring systems | --
S133 | Main harness near C102 | Harness Routing Views in wiring systems | --
S135 | Engine harness near the C104 breakout | Harness Routing Views in wiring systems | --
S201 (4-Door) | Instrument panel harness approximately at the C211 breakout | Harness Routing Views in wiring systems | --
S202 (4-Door) | Main harness approximately 15 cm (5.90 in) from the G200 breakout | Harness Routing Views in wiring systems | --
S203 | Main harness approximately 2 cm (0.78 in) from the blower motor resistor connector breakout | Harness Routing Views in wiring systems | --
S204 | Instrument panel harness approximately at the C211 breakout | Harness Routing Views in wiring systems | --
S205 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in wiring systems | --
S206 | Main harness approximately 20 cm (7.87 in) from the ignition switch connector breakout | Harness Routing Views in wiring systems | --
S208 | Main harness approximately 18 cm (7.08 in) from the ignition switch connector breakout | Harness Routing Views in wiring systems | --
S209 | Main harness approximately 12 cm (4.72 in) from the blower speed selector switch connector breakout | Harness Routing Views in wiring systems | --
S210 | Main harness approximately 12 cm (4.72 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S212 | Main harness approximately 6 cm (2.36 in) from the blower speed selector switch connector breakout | Harness Routing Views in wiring systems | --
S214 | Main harness approximately 10 cm (3.93 in) from the breakout. | Harness Routing Views in wiring systems | --
S216 | Main harness approximately 2 cm (0.78 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S218 | Main harness near the G200 breakout | Harness Routing Views in wiring systems | --
S219 | Main harness approximately 10 cm (3.93 in) from the daytime running lamps (DRL) control module connector breakout | Harness Routing Views in wiring systems | --
S220 | Main harness approximately 1 cm (0.93 in) from the blower speed selector switch connector breakout | Harness Routing Views in wiring systems | --
S221 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views in wiring systems | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views in wiring systems | --
S225 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter | Harness Routing Views in wiring systems | --
S226 | Instrument panel harness approximately at the radio breakout | Harness Routing Views in wiring systems | --
S227 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S228 | Main harness approximately 4 cm (1.57 in) from the C212 breakout | Harness Routing Views in wiring systems | --
S229 | Main harness approximately 7 cm (2.75 in) from the ignition switch connector breakout | Harness Routing Views in wiring systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in wiring systems | --
S234 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views in wiring systems | --
S236 (with Rear Wiper) | Instrument panel harness approximately 3 cm (1.18 in) from the C201 breakout | Harness Routing Views in wiring systems | --
S240 (4-Door) | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S247 | Main harness approximately 2 cm (0.78 in) from the C212 breakout | Harness Routing Views in wiring systems | --
S250 | Main harness approximately 5 cm (1.96 in) from the blower motor resistor connector breakout | Harness Routing Views in wiring systems | --
S251 | Main harness approximately 5 cm (1.96 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S254 | Main harness approximately 10 cm (3.93 in) from the G200 breakout | Harness Routing Views in wirng systems | --
S259 | A/C jumper harness behind the RH instrument panel near the A/C amplifier | Harness Routing Views in wiring systems | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S270 (with ABS) | Main harness approximately 12 cm (4.72 in) from the electronic brake control module (EBCM) connector C2 breakout | Harness Routing Views in wiring systems | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views in wiring systems | --
S275 | Main harness approximately 11 cm (4.33 in) from the ignition switch connector breakout | Harness Routing Views in wiring systems | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in wiring systems | --
S278 (with ABS) | Main harness approximately 14 cm (5.51 in) from the G200 breakout | Harness Routing Views in wiring systems | --
S284 | Main harness approximately 7 cm (2.75 in) from the C216 breakout | Harness Routing Views in wiring systems | --
S285 | Main harness approximately 10 cm (3.93 in) from the daytime running lamps (DRL) control module breakout | Harness Routing Views in wiring systems | --
S286 | Main harness approximately 6 cm (2.36 in) from the C216 breakout | Harness Routing Views in wiring systems | --
S296 | Main harness approximately 6 cm (2.36 in) from the stoplamp switch connector breakout | Harness Routing Views in wiring systems | --
S297 | Main harness approximately 5 cm (1.96 in) from the daytime running lamps (DRL) diode connector breakout | Harness Routing Views in wiring systems | --
S298 | Main harness approximately 2 cm (0.78 in) from the G200 breakout | Harness Routing Views in wiring systems | --
S299 | Main harness approximately 6 cm (2.36 in) from P201 | Harness Routing Views in wiring systems | --
S301 (2-Door) | Sub-floor harness near the seat belt switch connector breakout | Harness Routing Views in wiring systems | --
S306 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views in wiring systems | --
S400 | Rear door harness near G400 breakout | Harness Routing Views in wiring systems | --
S401 | Rear lamp harness, near LH rear combination lamp | Harness Routing Views in wiring systems | --
S402 | Rear lamp harness, near RH rear combination lamp | Harness Routing Views in wiring systems | --
S403 | Rear lamp harness near the RH rear combination lamp | Harness Routing Views in wiring systems | --
S404 (2-Door) | Floor harness approximately 4 cm (1.57 in) from the C406 breakout | Harness Routing Views in wiring systems | --
S404 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the LH rear speaker connector breakout | Harness Routing Views in wiring systems | --
S405 | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in wiring systems | --
S406 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views in wiring systems | --
S414 | LH rear combination lamp jumper near the LH rear combination lamp | Harness Routing Views in wiring systems | --
S415 | RH rear combination lamp jumper near the RH rear combination lamp | Harness Routing Views in wiring systems | --
S426 (4-Door) | Floor harness approximately 20 cm (7.87 in) from the G300 breakout | Harness Routing Views in wiring systems | --
S501 | LH front door power accessory harness near the LH front power window/ door lock switch connector breakout | Harness Routing Views in wiring systems | --
SP370 | Floor harness under the rear center console | Harness Routing Views in wiring systems | --