Master Electrical Component List. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Amplifier | Behind the RH instrument panel on the evaporator | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Compressor Clutch | LH front engine compartment attached to the A/C compressor | HVAC Component Views in HVAC System - Manual | --
A/C Compressor Clutch Relay | RH engine compartment near fuse block 1 | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Condenser Fan | Between the grille and the radiator | HVAC Component Views in HVAC System - Manual | --
A/C Condenser Fan Relay | RH Engine compartment near fuse block 1 | HVAC Component Views in HVAC System - Manual | HVAC Connector End Views in HVAC System - Manual
A/C Switch | Center of the instrument panel above the radio | -- | --
A/C Switch Fuse | RH instrument panel behind the instrument panel compartment | -- | --
Accelerometer (with ABS) | Under the center console | -- | --
Airbag Fuse Box | Under the left hand instrument panel near fuse block 2 | -- | --
Antilock Brake System (ABS) Motor Pack Assembly | LH rear engine compartment | Antilock Brake System Component Views in ABS | --
Audio Alarm Module | Behind the RH instrument panel near the RH front speaker | -- | --
Battery | RH rear engine compartment behind the strut | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | Data Link Communications Connector End Views in Instrument Panel, Gauges, and Console
Backup Lamp Switch (Manual Transmission) | Mounted on the top of the transmission | -- | --
Blower Motor | Behind the RH instrument panel | Heater Blower Controls Component Views in HVAC - Heating, Ventilation and Air Conditioning | --
Blower Motor Resistor | Behind the RH instrument panel on the top of the blower motor housing | Heater Blower Controls Component Views in HVAC - Heating, Ventilation and Air Conditioning | --
Blower Speed Selector Switch | Center of the instrument panel above the radio | Heater Blower Controls Component Views in HVAC - Heating, Ventilation and Air Conditioning | Heater Blower Controls Connector End Views in HVAC - Heating, Ventilation and Air Conditioning
Brake Fluid Level Switch | LH rear of the engine compartment in the brake F1 | Engine Controls Component Views in Engine Controls -1.6L | --
Camshaft Position Sensor | Inside the distributor to the rear of the engine | -- | --
Cigar Lighter | Center of the instrument panel below the radio | -- | --
Clutch Pedal Position (CPP) Switch (Manual Transmission) | Behind the LH instrument panel above the powertrain control module | -- | --
Clutch Pedal Position (CPP) Interrupt Switch (Manual Transmission with Cruise Control) | Under the LH instrument panel mounted to the clutch pedal bracket | Cruise Control Component Views in Cruise Control Component Views | --
Combination Switch | On the steering column | Power and Grounding Component Views | --
Crankshaft Position Sensor | Lower front of the engine in front of the oil pan | -- | --
Cruise Control Actuator | RH engine compartment near the strut tower | Cruise Control Component Views in Cruise Control Component Views | --
Cruise Control ON/OFF Switch | LH instrument panel to the right of the steering column | Cruise Control Component Views in Cruise Control Component Views | --
Cruise Control Mode Switch | RH steering column on the combination switch | -- | --
Data Link Connector - On Board Diagnostics II (DLC-OBDII) | LH instrument panel to the left of the center console of the knee bolster | Data Link Communications Component Views | Data Link Communications Component Views
Daytime Running Lamps (DRL) Control Module | Behind the instrument panel to the left of the steering column on the powertrain module mounting bracket | -- | --
Daytime Running Lamps (DRL) Diode | RH instrument panel taped to the main harness above the blower | -- | --
Diode Number 2 | Main harness behind the instrument panel compartment tape | -- | --
Distributor | Top rear of the engine | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Dome Lamp Diode (2 door) | Taped to the floor harness near C407 | Lighting Systems Component Views in Lighting Systems | --
Dome Lamp Diode (4 door) | Taped to the floor harness near C407 | Lighting Systems Component Views in lighting systems | --
Dual Pressure Switch | RH front engine compartment behind the radiator | HVAC Component Views in HVAC System - Manual | --
Duty Check Data Link Connector (DLC) 1 | RH engine compartment behind the RH headlamp | Data Link Communications Component Views | --
Duty Check Data Link Connector (DLC) 2 (4-speed automatic) | RH engine compartment behind the RH headlamp | -- | --
Electronic Brake Control Module (EBCM) (with ABS) | Under the LH instrument panel to the right of the steering column | Antilock Brake System Component Views in ABS | --
C1 (32 Cavities) | Main harness to the EBCM behind the instrument panel to the right of the steering column | -- | --
C2 (2 Cavities) | Main harness to the EBCM behind the instrument panel to the right of the steering column | -- | --
Electronic Brake Control Relay | LH engine compartment mounted to the left inner fender in front of the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
Engine Coolant Temperature (ECT) Sending Unit | RH side of the engine in the thermostat housing | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
Engine Coolant Temperature (ECT) Sensor | RH side of the engine in the thermostat housing | Engine Controls Component Views in Engine Controls -1.6L | --
Engine Coolant Temperature (ECT) Switch | RH side of the engine in the thermostat housing | Engine Controls Component Views in Engine Controls -1.6L | --
Evaporative (EVAP) Canister Purge Valve | RH front of the engine on the intake manifold | Engine Controls Component Views in Engine Controls -1.6L | --
Evaporative (EVAP) Canister Vent Control Valve | RH engine compartment near fuse block 1 | -- | --
Evaporative (EVAP) Tank Pressure Control Solenoid Vacuum | RH engine compartment near fuse block 1 | -- | --
Evaporator Thermistor | Behind the RH instrument panel in the evaporator housing | -- | --
Exhaust Gas Recirculation (EGR) Bypass Valve | RH front of the engine on the intake manifold | Engine Controls Component Views in Engine Controls -1.6L | --
Exhaust Gas Recirculation (EGR) Solenoid Vacuum Valve | RH front of the engine on the intake manifold | Engine Controls Component Views in Engine Controls -1.6L | --
Four Wheel Drive Low Switch (4-speed Automatic Transmission) | Top of the transfer case | -- | --
Four Wheel Drive Switch (3-speed Automatic Transmission) | Top of the transfer case | Antilock Brake System Component Views in ABS | --
Four Wheel Drive Switch (4-speed Automatic Transmission) | Top of the transfer case | -- | --
Four Wheel Drive Switch (Manual Transmission) | Top of the transfer case | Antilock Brake System Component Views in ABS | --
Front Washer Pump | RH front of the engine compartment on washer F1 | Wiper/Washer Component Views in Wipers/ Washer System | --
Front Wiper Motor | LH rear engine compartment on the bulkhead | Wiper/Washer Component Views in Wipers/ Washer System | --
Front Wipers/ Washers Switch | RH steering column in the combination switch | -- | --
Fuel Injector #1 | Top RH side of the engine | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Injector #2 | Top RH side of the engine | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Injector #3 | Top RH side of the engine | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Injector #4 | Top RH side of the engine | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Level Sensor | In the fuel tank | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Pump | In the fuel tank | Engine Controls Component Views in Engine Controls -1.6L | --
Fuel Pump Relay | Center of the instrument panel behind the blower speed selector | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls -1.6L
Fuel Tank Pressure Sensor | In the fuel tank | Engine Controls Component Views in Engine Controls -1.6L | --
Fuse Block 1 | RH engine compartment in front of the battery | Power and Grounding Component Views | --
C1 (3 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views | --
C2 (1 Cavities) | A/C harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views | --
C3 (1 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views | --
C4 (2 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views | --
Generator | RH lower front of the engine | -- | --
Headlamp/ Dimmer Switch | LH steering column in the combination switch | -- | --
Headlamp Relay 1 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views in Lighting Systems | --
Headlamp Relay 2 | RH instrument panel behind the instrument panel compartment in front of the blower motor | Lighting Systems Component Views in Lighting Systems | --
Heated Oxygen Sensor 1 (HO2S1) | LH rear of the engine in the exhaust manifold | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls -1.6L
Heated Oxygen Sensor 2 (HO2S2) | Below the vehicle after the 3-way catalytic converter (TWC) | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls -1.6L
Horn Relay | Center instrument panel behind the blower speed selector | Horn Component Views in Horns | --
Idle Air Control (IAC) Valve | RH engine below the throttle body | -- | --
Ignition Coil | Inside the distributor to the rear of the engine | -- | --
Ignition Key Warning Switch | RH side of the steering column on the ignition switch | -- | --
Ignition Switch | On the steering column | Power and Grounding Component Views | --
Illumination Controller | LH instrument panel to the left of the steering column | -- | SIR Connector End Views in SIR
Inflatable Restraint I/P Module | Top of the RH instrument panel above the instrument panel compartment | -- | SIR Connector End Views in SIR
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Under the center of the instrument panel | -- | SIR Connector End Views in SIR
Inflatable Restraint Steering Wheel Module | In the steering wheel | -- | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C1 (16 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C2 (10 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | --
Intake Air Temperature (IAT) Sensor | RH front of the engine below the throttle body | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Lamp Driver Relay | LH engine compartment mounted to the left inner fender in the front of the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
Left Front Wheel Speed Sensor (with ABS) | LH front wheel on the steering knuckle | Antilock Brake System Component Views in ABS | --
Left Horn | Between the grille and the radiator | Wiper/Washer Component Views in Wipers/ Washer Systems | --
LH Door Jamb Switch (2 Door) | Lower the LH B-Pillar | Lighting Systems Component Views in Lighting Systems | --
LH Horn Switch | LH side of the steering wheel | -- | --
LH Front ABS Solenoid | LH rear engine compartment attached to the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
LH Front Door Jamb Switch (4-Door) | Lower LH B-pillar | Lighting Systems Component Views in Lighting Systems | --
LH Front Power Door Lock Actuator Assembly (4-Door) | LH front power door on the door latch assembly | Power Door Systems Component Views in Doors | --
C1 (3 Cavities) | LH front door, LH front door harness to the LH front power door latch actuator | -- | --
C2 (6 Cavities | LH front door, LH front door harness to the LH front power door latch actuator | -- | --
LH Front Power Mirror Assembly (4-Door) | Behind the LH side view mirror | -- | --
LH Front Power Window/ Door Lock Switch (4-Door) | LH front door in the armrest | -- | --
LH Front Power Window Motor (4-Door) | LH front door behind the trim panel near the armrest | Power Door Systems Component Views in Doors | --
LH Front Speaker | LH top of the instrument panel near the windshield | Entertainment Component Views in Entertainment | --
LH Rear Door Jamb Switch (4-Door) | LH C-pillar above the wheelhousing | Lighting Systems Component Views in Lighting Systems | --
LH Rear Power Door Lock Actuator (4-Door) | LH rear door on the door latch assembly | Power Door Systems Component Views in Doors | --
LH Rear Power Window Motor (4-Door) | LH rear door behind the trim panel near the armrest | Power Door Systems Component Views in Doors | --
LH Rear Speaker (2-Door) | LH rear quarter trim panel in front of the rear seat | Entertainment Component Views in Entertainment | --
LH Rear Speaker (4-Door) | LH rear quarter trim panel behind the rear seat | Entertainment Component Views in Entertainment | --
Main Relay | Center of the instrument panel behind the blower speed selector | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Manifold Absolute Pressure (MAP) Sensor | Rear engine compartment on the bulkhead | Engine Controls Component Views in Engine Controls -1.6L | --
Mass Air Flow (MAF) Sensor | LH front engine compartment on the air cleaner (ACL) housing | Engine Controls Component Views in Engine Controls -1.6L | --
Noise Suppressor Filter | LH rear engine compartment below the front wiper motor | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Oil Pressure Switch | LH engine above the oil filter | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gauges, and Consol | --
Overdrive Switch (4-Speed Automatic Transmission) | Center console mounted in the manual selector lever | -- | --
Parking Brake Switch | In the center console to the left of the parking brake | -- | --
Park/ Neutral Position (PNP) Switch (3-Speed Automatic Transmission) | RH side of the transmission | -- | --
C1 (2 Cavities) | Engine harness to PNP switch on RH side of the transmission | -- | --
C2 (4 Cavities) | Engine harness to PNP switch on the RH side of the transmission | -- | --
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
3-Speed Automatic and Manual Transmissions C1 (2 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C2 (4 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C3 (16 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
3-Speed Automatic and Manual Transmissions C4 (26 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
Power Door Lock Control Module (4-Door) | LH instrument panel behind the power mirror switch to the left of the steering column | Power Door Systems Component Views in Doors | --
Power Mirror Switch (4-Door) | LH instrument panel to the left of the steering column | Power Door Systems Component Views in Doors | --
Power/ Normal Switch (4-Speed Automatic Transmission) | In the center console to the right of the manual selector lever | -- | --
Power Steering Pressure Switch | Lower LH engine in the power steering pump | Engine Controls Component Views in Engine Controls -1.6L | --
Power Windows Circuit Breaker (4-Door) | LH instrument panel mounted to fuse block 2 | -- | --
Radio | Center of the instrument panel | Entertainment Component Views in Entertainment | --
Rear Defogger (4-Door) | In the rear window | -- | --
Rear Defogger Switch (4-Door) | LH instrument panel to the left of the steering column | -- | --
Rear Door Jamb Switch | LH bottom of the rear door jamb | Power Door Systems Component Views in Doors | --
Rear Door Power Door Lock Actuator Assembly (4-Door) | Rear door on the door latch assembly | -- | --
Rear Washer Pump (4-Door) | RH front engine compartment on the washer fluid reservoir | Wiper/Washer Component Views in Wiper/Washer Systems | --
Rear Wheel Speed Sensor (with ABS) | In the rear differential carrier | -- | --
Rear Wiper Motor (4-Door) | In the center of the rear door | Wiper/Washer Component Views in Wiper/Washer Systems | --
Rear Wiper/ Washer Switch (4-Door) | LH instrument panel to the right of the steering column | Power and Grounding Component Views | --
RH Door Jamb Switch (2-Door) | Lower RH B-pillar | Power Door Systems Component Views in Doors | --
RH Front ABS Solenoid | LH rear engine compartment attached to the ABS hydraulic motor pack assembly | Antilock Brake System Component Views in ABS | --
RH Front Door Jamb Switch (4-Door) | Lower RH B-pillar | -- | --
RH Front Power Door Lock Actuator Assembly (4-Door) | RH front door on the door latch assembly | -- | --
C1 (3 Cavities) | RH front door harness to the RH front power door lock actuator | Power Door Systems Component Views in Doors | --
C2 (6 Cavities) | RH front door harness to the RH front power door lock actuator | -- | --
RH Front Power Mirror Assembly (4-Door) | Behind the RH side view mirror | Power Door Systems Component Views in Doors | --
RH Front Power Window Motor (4-Door) | In the RH front door behind the trim panel near the armrest | -- | --
RH Front Power Window Switch (4-Door) | RH front door in the armrest | -- | --
RH Front Speaker | RH top of the instrument panel near the windshield | Entertainment Component Views in Entertainment | --
RH Horn Switch | RH side of the steering wheel | -- | --
RH Rear Door Jamb (4-Door) | RH C-pillar above the wheelhousing | -- | --
RH Rear Power Door Lock Actuator (4-Door) | RH rear door on the door latch assembly | -- | --
RH Rear Power Window Motor (4-Door) | RH rear door behind the trim panel near the armrest | Power Door Systems Component Views in Doors | --
RH Rear Power Window Switch (4-Door) | RH rear door behind the trim panel near the armrest | Power Door Systems Component Views in Doors | --
RH Rear Remote Power Window (4-Door) | RH rear of the center console | Power Door Systems Component Views in Doors | --
RH Rear Speaker (2-Door) | RH rear quarter trim panel in front of the rear seat | Entertainment Component Views in Entertainment | --
RH Rear Speaker (4-Door) | RH rear quarter trim panel behind the rear seat | Entertainment Component Views in Entertainment | --
Right Front Wheel Speed Sensor (with ABS) | RH front wheel mounted on the steering knuckle | Antilock Brake System Component Views in ABS | --
Seat Belt Switch | In the driver seat belt buckle on the driver's seat adjuster | -- | --
Shift Lock Relay (Automatic Transmission) | RH engine compartment in front of the battery | -- | --
Shift Lock Solenoid (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Shift Lock Solenoid Capacitor (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Shift Solenoid Number 1 (4-Speed Automatic Transmission) | In the transmission attached to the valve body | -- | --
Shift Solenoid Number 2 (4-Speed Automatic Transmission) | In the transmission attached to the valve body | -- | --
Shuttle Switch | LH rear engine compartment attached to the ABS hydraulic motor pack assembly | -- | --
Starter Motor | Lower RH side of the engine under the intake manifold | -- | --
Starter Solenoid | Lower RH side of the engine on the starter motor | -- | --
Stoplamp Switch | Under the LH instrument panel above the brake pedal | Lighting Systems Component Views in Lighting Systems | --
Supplemental Inflatable Restraint (SIR) Contact Coil | In the top of the steering column | -- | SIR Connector End Views in SIR
C1 (2 Cavities) | SIR harness to the SIR contact coil in the steering column | -- | --
C2 (2 Cavities) | SIR contact coil to the inflatable restraint | -- | --
C3 (1 Cavities) | SIR contact coil to the horn switches in the steering column | -- | --
Supplemental Inflatable Restraint (SIR) Data Link Connector (DLC) | LH instrument panel under the steering column | -- | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Throttle Position (TP) Sensor | On the throttle body | Engine Controls Component Views in Engine Controls -1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Torque Converter Clutch (TCC) Relay (3-Speed Automatic Transmission) | RH engine compartment in front of the battery | -- | --
Torque Converter Clutch (TCC) Solenoid (Automatic Transmission) | In the transmission attached to the valve body | -- | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of the transmission | -- | --
Turn/ Hazard Relay | Center instrument panel behind the blower speed selector | -- | HVAC Connector End Views in HVAC System
Vehicle Speed Sensor (VSS) (4-Speed Automatic Transmission) | LH side of the transmission in the adapter case | -- | --
C100 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views | --
C101 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views | --
C102 (6 Cavities) (3-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views | --
C102 (4 Cavities) (Manual and 4-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views | --
C103 (12 Cavities) (Manual and 4-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views | --
C104 (6 Cavities) (Manual and 3-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views | --
C104 (9 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views | --
C105 (12 Cavities) | Engine harness to the injector harness, RH front of the engine | Harness Routing Views | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views | --
C108 (4 Cavities) | Main harness to the A/C sub-harness behind the RH headlamp | Harness Routing Views | --
C109 (2 Cavities) | Main harness to the RH front wheel speed sensor jumper harness behind the RH headlamp | Harness Routing Views | --
C110 (2 Cavities) | Main harness to the LH front wheel speed sensor jumper harness behind the LH headlamp | Harness Routing Views | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views | --
C202 (22 Cavities) | Main harness to the floor harness, LH instrument panel near G200 | Harness Routing Views | --
C203 (6 Cavities) | Main harness to the floor harness, LH instrument panel near G200 | Harness Routing Views | --
C204 (6 Cavities) (4-Door) | Main harness to the LH front door harness, LH instrument panel near the A-pillar | Harness Routing Views | --
C205 (4 Cavities) (4-Door) | Main harness to the LH front door harness, LH instrument panel near the A-pillar | Harness Routing Views | --
C206 (6 Cavities) (4-Door) | Main harness to the RH front door harness, RH instrument panel near the A-pillar | Harness Routing Views | --
C207 (4 Cavities) (4-Door) | Main harness to the RH front door harness, RH instrument panel near the A-pillar | Harness Routing Views | --
C208 (5 Cavities) | Instrument panel harness to the SIR harness, LH instrument panel to the right of the steering column | Harness Routing Views | --
C209 (3 Cavities) (4-Door) | Instrument panel harness to the LH front door harness, LH instrument panel near the A-pillar | Harness Routing Views | --
C210 (3 Cavities) (4-Door) | Instrument panel harness to the RH front door harness, RH instrument panel near the A-pillar | Harness Routing Views | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views | --
C212 (10 Cavities) | Main harness to the A/C amplifier jumper harness, RH instrument panel behind the instrument panel compartment | Harness Routing Views | --
C213 (6 Cavities) | Instrument panel harness to the shift illumination | Harness Routing Views | --
C215 (2 Cavities) (4-Door) | Main harness to the dome lamp harness, RH instrument panel near the A-pillar | Harness Routing Views | --
C217 (6 Cavities) | Main harness to the blower speed selector switch, RH instrument panel | Harness Routing Views | --
C300 (2 Cavities) (2-Door) | Floor harness to the dome lamp harness behind the LH rear passenger compartment trim panel | Harness Routing Views | --
C301 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views | --
C302 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views | --
C304 (3 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views | --
C305 (3 Cavities) (4-Door) | Floor harness to the LH rear door harness, LH B-pillar | Harness Routing Views | --
C306 (3 Cavities) (4-Door) | Floor harness to the RH rear door harness, RH B-pillar | Harness Routing Views | --
C307 (2 Cavities) (4-Door) | Floor harness to the LH rear door harness, LH B-pillar | Harness Routing Views | --
C308 (2 Cavities) (4-Door) | Floor harness to the RH rear door harness, RH B-pillar | Harness Routing Views | --
C400 (12 Cavities) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views | --
C401 (6 Cavities) (2-Door) | Floor harness to the rear lamp harness behind the LH rear wheelhousing | Harness Routing Views | --
C402 (6 Cavities) | Rear lamp harness to the RH rear combination lamp jumper harness behind the RH rear wheelhousing | Harness Routing Views | --
C403 (2 Cavities) (2-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views | --
C404 (1 Cavity) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views | --
C405 (2 Cavities) (4-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the rear door to the left of the license plate lamp connector breakout | Harness Routing Views | --
C405 (2 Cavities) (2-Door) | Rear door harness to the center high mount stoplamp jumper harness inside the center rear door | Harness Routing Views | --
C406 (6 Cavities) | Floor harness to the LH rear combination lamp jumper harness behind the LH rear wheelhousing | Harness Routing Views | --
C407 (6 Cavities) | Floor harness to the trailer option harness behind the LH rear wheelhousing | Harness Routing Views | --
C408 (3 Cavities) (4-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views | --
C409 (4 Cavities) (4-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views | --
C410 (1 Cavity) (4-Door) | Rear lamp harness to the rear door harness behind the RH rear wheelhousing | Harness Routing Views | --
C411 (3 Cavities) (4-Door) | Rear lamp harness to the fuel pressure sensor jumper harness under the rear of the vehicle above the fuel tank | Harness Routing Views | --
C412 (3 Cavities) | Floor harness to the rear wheel speed sensor jumper harness behind the LH wheelhousing | Harness Routing Views | --
C500 (10 Cavities) (4-Door) | LH front door harness to the LH front door power accessory harness in the LH front door right of the handle | Harness Routing Views | --
C501 (3 Cavities) (4-Door) | LH front door harness to the LH power mirror jumper harness in the LH front door right of the handle | Harness Routing Views | --
C600 (10 Cavities) (4-Door) | RH front door harness to the RH front door power accessory harness in the RH front door to the left of the handle | Harness Routing Views | --
C601 (4 Cavities) (4-Door) | RH front door power accessory harness to the RH front power window jumper harness in the RH front door left of the handle | Harness Routing Views | --
C602 (2 Cavities) (4-Door) | RH front power window switch jumper harness to the RH front power window motor in the RH front door to the left of the handle | Harness Routing Views | --
G100 | LH front inner fender | Power and Grounding Component Views | --
G101 | On the bulkhead behind the distributor | Power and Grounding Component Views | --
G102 | RH rear of the engine near the distributor | Power and Grounding Component Views | --
G103 | RH rear engine compartment mounted to the intake manifold | Power and Grounding Component Views | --
G104 | RH front inner fender near the washer fluid reservoir | Power and Grounding Component Views | --
G105 (with ABS) | RH inner fender near the battery | Power and Grounding Component Views | --
G106 | RH inner fender near the battery | Power and Grounding Component Views | --
G107 | RH engine near the starter motor | Power and Grounding Component Views | --
G108 (with A/C) | RH inner fender near the battery | Power and Grounding Component Views | --
G109 | LH bulkhead near the front of the wiper motor | Power and Grounding Component Views | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views | --
G201 | Behind the RH instrument panel near the blower assembly | Power and Grounding Component Views | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views | --
G203 | Center instrument panel on the sensing and diagnostic module mounting bracket | Power and Grounding Component Views | --
G300 (4-Door) | LH rear passenger compartment behind the trim panel | Power and Grounding Component Views | --
G300 (2-Door) | LH rear passenger compartment behind the trim plate | Power and Grounding Component Views | --
G400 (4-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views | --
G400 (2-Door) | Inside the rear door near the license plate lamps | Power and Grounding Component Views | --
G401 (4-Door) | Rear door harness near the rear wiper motor on the door | Power and Grounding Component Views | --
G402 (2-Door) | Rear lamp harness behind the LH rear wheelhousing | Power and Grounding Component Views | --
G403 (4-Door) | Rear door harness near the rear wiper motor on the mounting bracket | Power and Grounding Component Views | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Harness Routing Views | --
P201 | RH rear engine compartment on the bulkhead near the battery | Harness Routing Views | --
P300 (2-Door) | LH A-pillar under the instrument panel behind the LH kick panel | Harness Routing Views | --
P301 (2-Door) | In the floor under the driver's seat under the carpet | Harness Routing Views | --
P301 (4-Door) | In the floor under the driver's seat under the carpet | Harness Routing Views | --
P400 (2-Door) | Rear door | Harness Routing Views | --
P400 (4-Door) | Rear door | Harness Routing Views | --
P401 | Rear of the vehicle to the right of the LH frame rail | Harness Routing Views | --
P402 | Rear of the vehicle to the left of the RH frame rail | Harness Routing Views | --
P403 | LH rear of the vehicle to the left of the LH frame rail | Harness Routing Views | --
P500 (4-Door) | LH front door | Harness Routing Views | --
P600 (4-Door) | RH front door | Harness Routing Views | --
P700 (4-Door) | LH rear door | Harness Routing Views | --
P800 (4-Door) | RH rear door | Harness Routing Views | --
S100 (with Cruise) | Main harness approximately 21 cm (8.26 in) from the front wiper motor connector breakout | Harness Routing Views | --
S101 | Main harness approximately 8 cm (3.14 in) from the intake air temperature (IAT) sensor connector breakout | Harness Routing Views | --
S102 | Main harness near P201 | Harness Routing Views | --
S103 | Main harness approximately 8 cm (3.14 in) from the right horn connectors breakout | Harness Routing Views | --
S104 | Main harness approximately 4 cm (1.57 in) from the front washer pump connector breakout | Harness Routing Views | --
S105 | Main harness, approximately 11 cm (4.33 in) from the RH headlamp connector breakout | Harness Routing Views | --
S106 | Main harness, approximately 10 cm (3.93 in) from the noise suppressor filter connector breakout | Harness Routing Views | --
S107 | Engine harness approximately 10 cm (3.93 in) from the C104 breakout | Harness Routing Views | --
S108 (4-Speed Automatic Transmission) | Transmission harness near 4WD switch breakout | Harness Routing Views | --
S109 | Main harness approximately 20 cm (7.87 in) from the intake air temperature (IAT) sensor connector breakout | Harness Routing Views | --
S110 | Outer A/C harness RH engine compartment near the strut tower | Harness Routing Views | --
S111 | Main harness approximately 9 cm (3.54 in) from P200 | Harness Routing Views | --
S112 | Main harness approximately 2 cm (0.78 in) from P200 | Harness Routing Views | --
S113 | Main harness approximately 3 cm (1.18 in) from G103 breakout | Harness Routing Views | --
S114 | Outer A/C harness RH engine compartment near the strut tower | Harness Routing Views | --
S115 | Main harness approximately 10 cm (3.93 in) from the evaporative canister vent control valve | Harness Routing Views | --
S116 | Main harness approximately 14 cm (5.51 in) from the LH bulkhead branch breakout | Harness Routing Views | --
S117 (with ABS) | Main harness approximately 4 cm (1.57 in) from P200 | Harness Routing Views | --
S118 | Main harness behind the RH headlamp | Harness Routing Views | --
S119 | Main harness behind the LH headlamp | Harness Routing Views | --
S120 | Main harness approximately 15 cm (5.90 in) from the G100 breakout | Harness Routing Views | --
S121 | Injector harness near the fuel injector number 4 breakout | Harness Routing Views | --
S122 | Engine harness approximately 4 cm (1.57 in) from the crankshaft position sensor connector breakout | Harness Routing Views | --
S123 | Main harness approximately 4 cm (1.57 in) from P200 | Harness Routing Views | --
S124 (with ABS) | Main harness approximately 13 cm (5.11 in) from P200 | Harness Routing Views | --
S125 | Engine harness approximately 4 cm (1.57 in) from the starter motor connector breakout | Harness Routing Views | --
S126 | Main harness near the noise suppressor filter breakout | Harness Routing Views | --
S127 | Main harness approximately 3 cm (1.18 in) from P200 | Harness Routing Views | --
S128 | Injector harness near the C105 breakout | Harness Routing Views | --
S129 | Injector harness near the idle air control (IAC) valve connector breakout | Harness Routing Views | --
S130 | Main harness approximately 20 cm (7.87 in) from the noise suppressor filter connector breakout | Harness Routing Views | --
S131 | Main harness approximately 19 cm (7.48 in) from P201 | Harness Routing Views | --
S132 | Main harness approximately 7 cm (2.75 in) from the noise suppressor filter connector breakout | Harness Routing Views | --
S133 | Main harness near C102 | Harness Routing Views | --
S134 | Main harness near the heated oxygen sensor 1 (HO2S1) connector breakout | Harness Routing Views | --
S135 | Engine harness near the C104 breakout | Harness Routing Views | --
S136 | Engine harness approximately 1 cm (0.39 in) from the distributor connector breakout | Harness Routing Views | --
S137 | Engine harness approximately 2 cm (0.78 in) from the C101 breakout | Harness Routing Views | --
S138 | Engine harness approximately 12 cm (4.72 in) from the distributor connector breakout | Harness Routing Views | --
S139 | Main harness approximately 10 cm (3.93 in) from the noise suppressor filter connector breakout | Harness Routing Views | --
S140 | Main harness approximately 6 cm (2.36 in) from the noise suppressor filter connector breakout | Harness Routing Views | --
S141 | Main harness approximately 11 cm (4.33 in) from P200 | Harness Routing Views | --
S142 (3-Speed Automatic Transmission) | Main harness approximately 8 cm (3.14 in) from P201 | Harness Routing Views | --
S143 | Main harness approximately 17 cm (6.69 in) from P200 | Harness Routing Views | --
S200 | Instrument panel harness approximately 1 cm (0.39 in) from the power mirror switch connector breakout | Harness Routing Views | --
S201 (4-Door) | Instrument panel harness approximately at the C211 breakout | Harness Routing Views | --
S202 (4-Door) | Main harness approximately 15 cm (5.90 in) from the G200 breakout | Harness Routing Views | --
S203 | Main harness approximately 2 cm (0.78 in) from the blower motor resistor connector breakout | Harness Routing Views | --
S204 | Instrument panel harness approximately at the C211 breakout | Harness Routing Views | --
S205 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views | --
S206 | Main harness approximately 20 cm (7.87 in) from the ignition switch connector breakout | Harness Routing Views | --
S207 | Main harness LH rear of the engine compartment | Harness Routing Views | --
S208 | Main harness approximately 18 cm (7.08 in) from the ignition switch connector breakout | Harness Routing Views | --
S209 | Main harness approximately 12 cm (4.72 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S210 | Main harness approximately 12 cm (4.72 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S211 (with ABS) | Main harness approximately 9 cm (3.54 in) from the electronic brake control module (EBCM) | Harness Routing Views | --
S212 | Main harness approximately 6 cm (2.36 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S213 | Main harness approximately 3 cm (1.18 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S214 | Main harness approximately 10 cm (3.93 in) from the | Harness Routing Views | --
S215 | Main harness near the powertrain control module (PCM) connector C2 breakout | Harness Routing Views | --
S216 | Main harness approximately 2 cm (0.78 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S217 | Main harness near the electronic brake control module (EBCM) connector breakout | Harness Routing Views | --
S218 | Main harness near the G200 breakout | Harness Routing Views | --
S219 | Main harness approximately 10 cm (3.93 in) from the daytime running lamps (DRL) control module connector breakout | Harness Routing Views | --
S220 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S221 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter breakout | Harness Routing Views | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S223 | Main harness near fuse block 2 | Harness Routing Views | --
S224 (3-Speed Automatic Transmission) | Main harness approximately 10 cm (3.93 in) from the ignition switch breakout | Harness Routing Views | --
S225 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter | Harness Routing Views | --
S226 | Instrument panel harness approximately at the radio breakout | Harness Routing Views | --
S227 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S228 | Main harness approximately 4 cm (1.57 in) from the C212 breakout | Harness Routing Views | --
S229 | Main harness approximately 7 cm (2.75 in) from the ignition switch connector breakout | Harness Routing Views | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views | --
S231 | Main harness approximately 1 cm (0.39 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S232 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views | --
S233 | Floor harness 1 near the LH rear wheelhousing | Harness Routing Views | --
S234 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views | --
S235 | Instrument panel harness approximately 1 cm (0.39 in) from the C211 breakout | Harness Routing Views | --
S236 (with Rear Wiper) | Instrument panel harness approximately 3 cm (1.18 in) from the C201 breakout | Harness Routing Views | --
S237 | Main harness near the powertrain control module (PCM) connector breakout | Harness Routing Views | --
S238 | Instrument harness approximately 2 cm (0.78 in) from the C209 breakout | Harness Routing Views | --
S239 | Main harness approximately 2 cm (0.78 in) from the daytime running lamps (DRL) diode breakout | Harness Routing Views | --
S240 (4-Door) | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S241 | Main harness approximately 8 cm (3.14 in) from the powertrain control module (PCM) connectors breakout | Harness Routing Views | --
S242 | Main harness near the G200 breakout | Harness Routing Views | --
S243 | Main harness approximately 17 cm (6.69 in) from the G216 breakout | Harness Routing Views | --
S244 | Main harness approximately 25 cm (9.84 in) from the ignition switch connector breakout | Harness Routing Views | --
S245 | Floor harness near the C211 connector breakout | Harness Routing Views | --
S246 | Main harness approximately 14 cm (5.51 in) from the ignition switch connector breakout | Harness Routing Views | --
S247 | Main harness approximately 2 cm (0.87 in) from the C212 breakout | Harness Routing Views | --
S248 (Manual Transmission) | Main harness approximately 13 cm (5.11 in) from the steering column branch breakout | Harness Routing Views | --
S249 | Main harness left of the steering column | Harness Routing Views | --
S250 | Main harness approximately 5 cm from the blower motor resistor connector breakout | Harness Routing Views | --
S251 | Main harness approximately 5 cm (1.96 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S252 (with Cruise) | Main harness approximately 3 cm (1.18 in) from the steering column breakout | Harness Routing Views | --
S253 | Main harness approximately 3 cm (1.18 in) from the headlamp relay 1 and headlamp relay 2 breakouts | Harness Routing Views | --
S254 | Main harness approximately 10 cm (3.93 in) from the G200 breakout | Harness Routing Views | --
S255 | Main harness approximately 16 cm (6.29 in) from the ignition switch connector breakout | Harness Routing Views | --
S256 | Instrument panel harness approximately 3 cm (1.18 in) from the power mirror switch connector breakout | Harness Routing Views | --
S257 | Main harness approximately 1 cm (0.39 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S258 | Instrument panel harness approximately 2 cm (0.78 in) from the power mirror switch connector breakout | Harness Routing Views | --
S259 | A/C jumper harness behind the RH instrument panel near the A/C amplifier | Harness Routing Views | --
S260 | Main harness approximately 4 cm (1.57 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S261 | Main harness near the C212 connector breakout | Harness Routing Views | --
S262 | Main harness approximately 8 cm (3.14 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S263 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views | --
S264 | Main harness approximately 18 cm (7.08 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S265 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views | --
S266 | Main harness approximately 8 cm (3.14 in) from the C204 breakout | Harness Routing Views | --
S267 | Main harness approximately 4 cm (1.57 in) from the stoplamp switch breakout | Harness Routing Views | --
S268 (4-Door) | Main harness approximately 3 cm (1.18 in) from the G200 breakout | Harness Routing Views | --
S269 | Main harness approximately 8 cm (3.14 in) from the C204 breakout | Harness Routing Views | --
S270 (with ABS) | Main harness approximately 12 cm (4.72 in) from the electronic brake control module (EBCM) connector C2 breakout | Harness Routing Views | --
S271 (with ABS) | Main harness approximately 2 cm (0.78 in) from the C212 breakout | Harness Routing Views | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views | --
S273 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S274 (3-Speed Automatic Transmission) | Main harness approximately 3 cm (1.18 in) from the powertrain control module (PCM) connector breakout | Harness Routing Views | --
S275 | Main harness approximately 11 cm (4.33 in) from the ignition switch connector breakout | Harness Routing Views | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views | --
S277 (3-Speed Automatic Transmission) | Main harness approximately 2 cm (0.78 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S278 (with ABS) | Main harness approximately 14 cm (5.51 in) from the G200 breakout | Harness Routing Views | --
S279 | Main harness approximately 3 cm (1.18 in) from the powertrain control module (PCM) connector breakout | Harness Routing Views | --
S280 | Main harness approximately 3 cm (1.18 in) from the powertrain control module (PCM) connector breakout | Harness Routing Views | --
S281 | Main harness approximately 3 cm (1.18 in) from the C203 breakout | Harness Routing Views | --
S282 | Main harness near G200 breakout | Harness Routing Views | --
S283 | Main harness approximately 8 cm (3.14 in) from the daytime running lamps (DRL) control module connector breakout | Harness Routing Views | --
S284 | Main harness approximately 7 cm (2.75 in) from the C216 breakout | Harness Routing Views | --
S285 | Main harness approximately 10 cm (3.93 in) from the daytime running lamps (DRL) control module breakout | Harness Routing Views | --
S286 | Main harness approximately 6 cm (2.36 in) from the C216 breakout | Harness Routing Views | --
S287 | Main harness approximately 4 cm (1.57 in) from the C203 breakout | Harness Routing Views | --
S288 | Main harness approximately 2 cm (0.78 in) from the G200 breakout | Harness Routing Views | --
S289 (3-Speed Automatic Transmission) | Main harness approximately 2 cm (0.78 in) from the powertrain control module (PCM) connectors breakout | Harness Routing Views | --
S290 | Main harness to the left of the steering column | Harness Routing Views | --
S291 (4-Speed Automatic Transmission) | Main harness near the powertrain control module (PCM) | Harness Routing Views | --
S292 | Main harness near P200 | Harness Routing Views | --
S293 | Main harness near the G200 breakout | Harness Routing Views | --
S294 | Main harness approximately 10 cm (3.93 in) from the G20 breakout | Harness Routing Views | --
S295 | Main harness approximately 7 cm (2.75 in) from the blower speed selector switch connector breakout | Harness Routing Views | --
S296 | Main harness approximately 6 cm (2.36 in) from the stoplamp switch connector breakout | Harness Routing Views | --
S297 | Main harness approximately 5 cm (1.96 in) from the daytime running lamps (DRL) diode connector breakout | Harness Routing Views | --
S298 | Main harness approximately 2 cm (0.78 in) from the G200 breakout | Harness Routing Views | --
S299 | Main harness approximately 6 cm (2.36 in) from P201 | Harness Routing Views | --
S300 (2-Door) | Floor harness approximately 10 cm (3.93 in) from the LH rear speaker connector breakout | Harness Routing Views | --
S301 (2-Door) | Sub-floor harness near the seat belt switch connector breakout | Harness Routing Views | --
S302 (4-Door) | Floor harness near the heated oxygen sensor 2 (HO2S2) connector breakout | Harness Routing Views | --
S303 (4-Door) | Floor harness near the heated oxygen sensor 2 (HO2S2) connector breakout | Harness Routing Views | --
S304 (2-Door) | Floor harness approximately 5 cm (1.96 in) from the LH rear speaker connector breakout | Harness Routing Views | --
S305 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views | --
S306 (2-Door) | Floor harness approximately 20 cm (7.87 in) from the LH rear speaker connector breakout | Harness Routing Views | --
S310 | Floor harness near the dome lamp diode breakout | Harness Routing Views | --
S350 | Floor harness near the RH rear door jamb switch breakout | Harness Routing Views | --
S351 | Floor harness near the G300 breakout | Harness Routing Views | --
S400 | Rear door harness near G400 breakout | Harness Routing Views | --
S401 | Rear lamp harness, near LH rear combination lamp | Harness Routing Views | --
S402 | Rear lamp harness, near RH rear combination lamp | Harness Routing Views | --
S403 | Rear lamp harness near the RH rear combination lamp | Harness Routing Views | --
S404 (2-Door) | Floor harness approximately 4 cm (1.57 in) from the C406 breakout | Harness Routing Views | --
S404 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the LH rear speaker connector breakout | Harness Routing Views | --
S405 | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views | --
S406 (4-Door) | Floor harness approximately 4 cm (1.57 in) from the G300 breakout | Harness Routing Views | --
S407 | Rear door harness near the license plate lamps | Harness Routing Views | --
S408 | Rear lamp harness near the LH rear combination lamp | Harness Routing Views | --
S409 (2-Door) | Floor harness approximately 5 cm (1.96 in) from the C406 breakout | Harness Routing Views | --
S409 (4-Door) | Floor harness approximately 30 cm (11.81 in) from the G300 breakout | Harness Routing Views | --
S410 | Rear door harness near the license plate lamps | Harness Routing Views | --
S411 (2-Door) | Floor harness approximately 2 cm (0.78 in) from the C406 breakout | Harness Routing Views | --
S411 (4-Door) | Floor harness approximately 2 cm (0.78 in) from the G300 breakout | Harness Routing Views | --
S412 (4-Door) | Floor harness approximately 42 cm (16.53 in) from the G300 breakout | Harness Routing Views | --
S413 (2-Door) | Floor harness approximately 10 cm (3.93 in) from the C406 breakout | Harness Routing Views | --
S413 (4-Door) | Floor harness approximately 30 cm (11.81 in) from the G300 breakout | Harness Routing Views | --
S414 | LH rear combination lamp jumper near the LH rear combination lamp | Harness Routing Views | --
S415 | RH rear combination lamp jumper near the RH rear combination lamp | Harness Routing Views | --
S416 | Rear lamp harness near the RH rear combination lamp connector breakout | Harness Routing Views | --
S417 | Floor harness 1 near the LH rear wheel housing | Harness Routing Views | --
S418 (2-Door) | Floor harness approximately 3 cm (1.18 in) from the C406 breakout | Harness Routing Views | --
S418 (4-Door) | Floor harness approximately 25 cm (9.84 in) from the G300 breakout | Harness Routing Views | --
S419 (4-Door) | Floor harness approximately 50 cm (19.68 in) from the G300 breakout | Harness Routing Views | --
S420 (4-Door) | Floor harness approximately 53 cm (20.86 in) from the G300 breakout | Harness Routing Views | --
S421 (4-Door) | Floor harness approximately 40 cm (15.74 in) from the G300 breakout | Harness Routing Views | --
S422 (4-Door) | Floor harness approximately 7 cm (2.75 in) from the G300 breakout | Harness Routing Views | --
S423 (4-Door) | Floor harness approximately 8 cm (3.14 in) from the G300 breakout | Harness Routing Views | --
S424 (4-Door) | Floor harness approximately 10 cm (3.93 in) from the C406 breakout | Harness Routing Views | --
S425 (4-Door) | Floor harness approximately 50 cm (19.68 in) from the G300 breakout | Harness Routing Views | --
S426 (4-Door) | Floor harness approximately 20 cm (7.87 in) from the G300 breakout | Harness Routing Views | --
S501 | LH front door power accessory harness near the LH front power window/ door lock switch connector breakout | Harness Routing Views | --
S502 | LH front door power accessory harness near the LH front power window/ door lock switch connector breakout | Harness Routing Views | --
S503 | LH front door power accessory harness near the LH front power window/ door lock switch connector breakout | Harness Routing Views | --
S504 | LH front door harness near the C500 breakout | Harness Routing Views | --
S604 | RH front door harness near the C600 breakout | Harness Routing Views | --
SP370 (Power Windows) | Floor harness under the rear center console | Harness Routing Views | --
SP371 (Power Windows) | Floor harness under the rear center console | Harness Routing Views | --