Door Sill Plate Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

## Door Sill Plate Replacement Front

### Removal Procedure

1. Remove the 3 screws from the front sill plate.
2. Remove the front sill plate.

### Installation Procedure

Install the front sill plate to the vehicle. Secure the front sill plate with the 3 screws.

## Door Sill Plate Replacement Rear

### Removal Procedure

1. Remove the 2 screws from the rear sill plate (4).
2. Remove the rear sill plate.

### Installation Procedure

Install the rear sill plate (4) to the vehicle. Secure the rear sill plate with the 2 screws.