Brake Band, Reaction Sun Gear, and Reaction Drum Assembly Installation. Pontiac Sun Runner - 4WD (Canada) 1997

For 1990-2009 cars

### Tools Required

J 36850 Transjel®

1. Install the brake band (404).
2. Install the reaction sun gear thrust washer and lower reaction sun gear bearing (401). The case bushing acts as a guide for the thrust washer and bearing.
3. Install the reaction sun gear and drum assembly (403).
4. Install the upper reaction sun gear bearing and thrust washer (401). Retain with J 36850 or equivalent.