Trim Cover Replacement - Center Rocker Panel. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 4 screws which secure the rocker panel center trim cover (3).
2. Lift the rocker panel center trim cover (3) off the center retainer (1).
3. Remove the cover (3) from the rocker panel.

### Installation Procedure

Install the rocker panel center trim cover (3) to the center retainer (1). Secure the trim cover to the rocker panel with the 4 screws.