Fastener Tightening Specifications. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Booster Assembly Mounting Nuts | 13 N·m | 115 lb in
Brake Pipe Fitting Nuts | 16 N·m | 12 lb ft
Brake Pedal Pivot Shaft Bolt Nut | 30 N·m | 22 lb ft
Caliper Union Bolt | 23 N·m | 17 lb ft
Load Sensing Spring Bolt | 23 N·m | 17 lb ft
Load Sensing Spring Bracket Bolts | 23 N·m | 17 lb ft
Load Sensing Proportioning Valve (LSPV) Assembly Bolts | 23 N·m | 17 lb ft
Master Cylinder Brake Pipe Flare Nuts | 16 N·m | 12 lb ft
Master Cylinder Nuts | 13 N·m | 115 lb in
Piston Stopper Bolt | 10 N·m | 89 lb in
Push Rod Clevis Locknut | 26 N·m | 19 lb ft
Stoplamp Switch Locknut | 10 N·m | 89 lb in
Wheel Cylinder/Caliper Bleeder Valve | 16 N·m | 12 lb ft