Instrument Cluster Lens Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster assembly. Refer to Instrument Cluster Replacement .
2. Release the 7 plastic clear tabs in order to remove the lens (7) from the instrument cluster assembly (3).

### Installation Procedure

1. Install the lens (7) to the instrument cluster assembly (3) by pressing around the lens until the tabs snap into place.
2. Install the instrument cluster assembly to the instrument panel. Refer to Instrument Cluster Replacement .