Windshield Washer Solvent Container Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws and the washer fluid reservoir assembly (2) from the vehicle.
2. Disconnect the front washer pump electrical connector.
3. Disconnect the rear washer pump electrical connector, if equipped.
4. Remove the front washer hose (4) from the front washer pump (3).
5. Remove the rear washer hose from the rear washer pump, if equipped.
6. Remove the front washer pump (3) from the reservoir (2).
7. Remove the rear washer pump from the reservoir (2), if equipped.

### Installation Procedure

1. Install the front washer pump (3) to the washer fluid reservoir (2).
2. Install the rear washer pump to the rear washer fluid reservoir (2), if equipped.
3. Install the front washer hose (4) to the front washer pump (3).
4. Install the rear washer hose to the rear washer pump, if equipped.
5. Connect the front washer pump electrical connector.
6. Connect the rear washer pump electrical connector, if equipped.
7. Install the washer fluid reservoir (2) to the vehicle. Secure the reservoir with 2 screws.