SIR Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Airbag Fuse box | Under LH I/P, near Fuse Block 2 | -- | --
Combination Switch | On Steering Column | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views in Wiring Systems | --
Inflatable Restraint I/P Module | Top of RH I/P, above I/P Compartment | -- | SIR Connector End Views
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Under Center I/P | -- | SIR Connector End Views
Inflatable Restraint Steering Wheel Module | In Steering Wheel | -- | SIR Connector End Views
Instrument Panel Cluster Assembly | LH I/P | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Instrument Panel Cluster Assembly C! (16 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Instrument Panel Cluster Assembly C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Seat Belt Switch | In Driver Seat Belt Buckle, on Driver's Seat Adjuster | -- | --
C201 (16 Cavities) | Main Harness, to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views in Wiring Systems | --
C205 (4 Cavities) (4-Door) | Main Harness to LH Front Door Harness, LH I/P, near A-Pillar | Harness Routing Views in Wiring Systems | --
C208 (5 Cavities) | I/P Harness to SIR Harness, LH I/P, right of Steering Column | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | I/P Harness to Floor Harness, LH I/P, near A-Pillar | Harness Routing Views in Wiring Systems | --
C301 (6 Cavities) (4-Door) | Floor Harness to Sub-Floor Harness, behind LH Rear Passenger Compartment Trim Panel | -- | --
C306 (3 Cavities) (4-Door) | Floor Harness to RH Rear Door Harness, RH B-Pillar | Harness Routing Views in Wiring Systems | --
G203 | Center I/P, on Sensing and Diagnostic Module Mounting Bracket | Harness Routing Views in Wiring Systems | --
G300 | LH Rear Passenger Compartment, behind Trim Panel | -- | --
P300 | LH A-Pillar, under I/P, behind LH Kick Panel | Harness Routing Views in Wiring Systems | --
S204 | I/P Harness, approximately at C211 breakout | Harness Routing Views in Wiring Systems | --
S213 | Main Harness, approximately 3 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S301 (2-Door) | Sub-Floor Harness, near Seat Belt Switch Connector breakout | -- | --
S404 (2-Door) | Floor Harness, approximately 4 cm from C406 breakout | Harness Routing Views in Wiring Systems | --
S404 (4-Door) | Floor Harness, approximately 4 cm from LH Rear Speaker connector breakout | -- | --