Brake Backing Plate Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the wheel cylinder. Refer to Wheel Cylinder Replacement .
2. Remove the parking brake cable (3) from the backing plate (1) by squeezing the parking brake cable stopper ring (2).
3. Remove the axle shaft. Refer to Axle Shaft Replacement in Rear Drive Axle.

### Installation Procedure

1. Install the axle shaft. Refer to Axle Shaft Replacement in Rear Drive Axle.
2. Install the parking brake (3) to the backing plate (1).
3. Install the wheel cylinder. Refer to Wheel Cylinder Replacement in this section.