ABS Components. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Accelerometer (with ABS) | Under Center Console | -- | --
Antilock Brake System (ABS) Motor Pack Assembly | LH Rear Engine Compartment | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Electronic Brake Control Relay | LH Engine Compartment, mounted to Left Inner Fender in front of ABS Hydraulic Motor Pack Assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Antilock Brake System (ABS) Resistor | RH I/P, behind I/P Compartment taped to Main Harness | -- | Antilock Brake System Connector End Views
Brake Fluid Level Switch | LH rear of Engine Compartment in Brake Fluid Reservoir | Antilock Brake System Component Views | --
Diode No. 2 | Main Harness, behind I/P Compartment taped to harness | -- | --
Electronic Brake Control Module (EBCM) (with ABS) | Under LH I/P, right of Steering Column | Antilock Brake System Component Views | --
Electronic Brake Control Module (EBCM) (with ABS) C1 (32 Cavities) | Main Harness to EBCM, behind I/P right of Steering Column | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Electronic Brake Control Module (EBCM) (with ABS) C2 (2 Cavities) | Main Harness to EBCM, behind I/P right of Steering Column | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Four Wheel Drive Switch | Top of Transfer Case | -- | --
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 1 - C1 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 1 - C2 (1 Cavity) | A/C Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 1 - C3 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views in Wiring Systems | --
Instrument Panel Cluster Assembly | LH I/P | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Instrument Panel Cluster Assembly C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | --
Lamp Driver Relay | LH Engine Compartment, mounted to Left Inner Fender in front of ABS Hydraulic Motor Pack Assembly | Antilock Brake System Component Views in Lighting Systems | --
LH Front ABS Solenoid | LH Rear Engine Compartment attached to ABS Hydraulic Motor Pack Assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Left Front wheel Speed Sensor (with ABS) | LH Front Wheel, on Steering Knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Powertrain Control Module (PCM) | Under LH I/P, left of Steering Column | -- | --
Rear Wheel Speed Sensor (with ABS) | In Rear Differential Carrier | Antilock Brake System Component Views | Antilock Brake System Connector End Views
RH Front ABS Solenoid | LH Rear Engine Compartment attached to ABS Hydraulic Motor Pack Assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Right Front wheel Speed Sensor (with ABS) | RH Front Wheel, mounted on Steering Knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Shuttle Switch | LH Rear Engine compartment, attached to ABS Hydraulic Motor Pack Assembly | -- | --
Stoplamp Switch | Under LH I/P, above Brake Pedal | Lighting Systems Component Views in Lighting Systems | --
C100 (16 cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C104 (6 Cavities) (Manual and 3-Speed Automatic Transmissions) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views in Wiring Systems | --
C104 (9 Cavities) (4-Speed Automatic Transmission) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views in Wiring Systems | --
C109 (2 Cavities) | Main Harness to RH Front Wheel Speed Sensor Jumper Harness, behind RH Headlamp | Harness Routing Views in Wiring Systems | --
C110 (2 Cavities) | Main Harness to LH Front Wheel Speed Sensor Jumper Harness, behind LH Headlamp | Harness Routing Views in Wiring Systems | --
C200 (22 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main Harness to I/P Harness, LH I/P near fuse Block 2 | Harness Routing Views in Wiring Systems | --
C203 (6 Cavities) | Main Harness to Floor Harness, LH I/P near G200 | Harness Routing Views in Wiring Systems | --
C304 (3 Cavities) (2 Door) | Floor Harness to Sub-Floor Harness, behind LH Rear Passenger Compartment Trim Panel | -- | --
G101 | On Bulkhead behind Distributor | Harness Routing Views in Wiring Systems | --
G105 (with ABS) | RH Inner Fender, near Battery | Harness Routing Views in Wiring Systems | --
G200 | Behind LH I/P, above Fuse Block 2 | Harness Routing Views in Wiring Systems | --
G202 | Behind Center I/P on Bulkhead | -- | --
G300 (4-Door) | LH Rear Passenger Compartment, behind Trim Panel | Harness Routing Views in Wiring Systems | --
G300 (2-Door) | LH Rear Passenger Compartment, behind Trim Panel | Harness Routing Views in Wiring Systems | --
G400 | Inside Rear Door near License Plate Lamps | Harness Routing Views in Wiring Systems | --
G402 (2-Door) | Rear Lamp Harness, behind LH Rear Wheelhousing | -- | --
P200 | LH Rear Engine Compartment on Bulkhead, near Brake Master Cylinder | Harness Routing Views in Wiring Systems | --
P201 | RH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views in Wiring Systems | --
P300 (2-Door) | LH A-Pillar, under I/P, behind LH Kick Panel | Harness Routing Views in Wiring Systems | --
P403 | LH rear of Vehicle, Left of LH Frame Rail | Harness Routing Views in Wiring Systems | --
S106 | Main Harness, approximately 10 cm from Noise Suppressor Filter connector breakout | -- | --
S108 (4-Speed Automatic transmission) | Transmission Harness, near 4WD Switch breakout | -- | --
S204 | I/P Harness, approximately at C211 breakout | Harness Routing Views in Wiring Systems | --
S208 | Main Harness, approximately 18 cm from Ignition Switch connector breakout | Harness Routing Views in Wiring Systems | --
S211 (with ABS) | Main Harness, approximately 9 cm from Electronic Brake Control Module (EBCM) connector C2 breakout | Harness Routing Views in Wiring Systems | --
S213 | Main Harness, approximately 3 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S251 | Main Harness, approximately 5 cm from Stoplamp Switch connector breakout | -- | --
S254 | Main Harness, approximately 10 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S260 | Main Harness, approximately 4 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S262 | Main Harness, approximately 8 cm from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S270 (with ABS) | Main Harness, approximately 12 cm from Electronic Brake Control Module (EBCM) connector C2 breakout | Harness Routing Views in Wiring Systems | --
S271 (with ABS) | Main Harness, approximately 2 cm from C212 breakout | Harness Routing Views in Wiring Systems | --
S272 | Main Harness, approximately 11 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S275 | Main Harness, approximately 11 cm from Ignition Switch connector breakout | Harness Routing Views in Wiring Systems | --
S276 | Main Harness, approximately 1 cm from G200 breakout | -- | --
S278 (with ABS) | Main Harness, approximately 14 cm from G200 breakout | Harness Routing Views in Wiring Systems | --
S280 | Main Harness, approximately 3 cm from Powertrain Control Module (PCM) connector breakout | -- | --
S281 | Main Harness, approximately 3 cm from C203 breakout | -- | --
S298 | Main Harness, approximately 2 cm from G200 breakout | -- | --